|  |  |
| --- | --- |
| **Date:** | **Trainer: PAIGE METZ** |
| **Your Name: (print)** | **(Signature)** |
| **Employer: COUNTRY PUMP OUT** | **WHMIS Training: Yes No**  |

*(Please identify all correct answers)*

**1. What personal protective equipment (PPE) is required on site?**

1. Coveralls
2. CSA approved work boots
3. CSA approved safety glasses
4. CSA approved Class 1 hard hat

**2. What is the emergency phone number?**

**3. What does a cross hatched area indicate** (*yellow & black lines*) **when on a tour route?**

1. Nothing really
2. Hazard, you may pass but do not stop
3. A process viewing location

**4.** **When would you phone the emergency number?**

1. Injury
2. Environmental spill
3. Fire
4. Gas

**5.** **What are the correct muster points for a gas evacuation in Grande Prairie Lumber?**

1. Sawmill = Sawmill Basement
2. Planermill = Planermill 3rd Floor Conference Room
3. Sawmill = Sawmill Lunchroom
4. Planermill = Grading Office

**6.**  **Can you enter a “Caution Do Not Enter” yellow barrier taped off area if you are not part of the work crew working on the job inside?**

1. No
2. Yes

**7. Which of the following things do you have to know in the event of an evacuation?**

1. What area you are working in
2. The evacuation route from the area
3. Where the muster point is
4. Are you accounted for

**8.** **What are the correct muster points for a fire evacuation in Grande Prairie Lumber?**

1. Sawmill = Outside the west side of the Office Building
2. Planermill = Planermill Cafeteria
3. Sawmill = Sawmill Basement
4. Planermill = Weigh Scalehouse

**9. What are 2 key things you can do to help us comply with our environmental policy?**

 1.

 2.

**10. When is a safe work permit required?**

1. Confined space entry
2. Contractor work
3. Hot work
4. Vendor visits

**11. Which of the following are GP Lumber Safe Work permit requirements?**

1. White (first) copy placed on active board during work
2. Pink (second) copy is located at job site
3. Safe Work permit is canceled once work complete
4. During hot work, an additional Hot Work Permit must be posted at job site
5. Hot Work Permit is removed once the work is complete

**12. Safe Work Permits are used:**

1. To account for personnel in the event of an evacuation
2. As a checklist to ensure that equipment is safe to work on
3. As a checklist to identify the required PPE for the job
4. As an agreement between the Contractor and Weyerhaeuser

**13. Which of the following are Grande Prairie Lumber lockout requirements?**

1. More than one individual may work under a single lock
2. Only the owner may place or remove their personal lock
3. Locks must be removed (or tagged) prior to leaving site
4. Lock box is a storage box located in the lunchroom

**14. Which of the following are true of the lockbox process?**

1. Seal number on outside of the box must match the number recorded on the sheet inside box
2. To gain personal control of a lockbox, you must place your personal lock on it
3. It only requires one Weyerhaeuser individual to do a lockbox lockout

**15. What must you do if you are injured on site?**

1. Immediately report the injury to Weyerhaeuser
2. See a Standard First Aider as directed

c) Fill out appropriate documentation

d) Leave the site

**16. If you need to leave the site prior to shift end (i.e. feeling ill), what must you do?**

1. Inform your Supervisor
2. Inform your site contact and see a Standard First Aider if applicable
3. Remove any personal locks you have applied
4. Remove your name from the Safe Work permit

**17. What are you expected to do when approaching a rail crossing?**

1. Only stop if a train is present
2. Cross as a pedestrian if the train is closer than 200 feet
3. Stop when in a vehicle
4. All the above

**18. You can enter a confined space through any opening?**

1. True
2. False

**19. What are the 3 of our 6 Core Safety Values of our site?**

 1.

 2.

 3.

**20.** **I must take part in a field level hazard assessment prior to starting a task.**

1. True
2. False

**21. Hearing Protection must be worn in noise levels of 85 dBA or greater.**

1. True
2. False

**22.** **Name 2 Grande Prairie Lumber significant environmental aspects?**

 1.

 2.

**23**. **Safety Glasses must be worn in the front seat of all vehicles on site**

1. True
2. False

**24. What are GP lumber’s 3 Safety absolutes?**

1. Safe work plan
2. Lockout,
3. Fall protection,
4. Tampering with a safety device.

**25. What are your reasons for ensuring your personal safety while you work at GP Lumber?**

1. Family
2. Friends
3. Personal well being
4. Recreation
5. All the above & \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Scoring: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (must achieve 80% or greater)

Know Safety, No Pain

Know Pain, No Safety

